******** BSIM-MG 105 Sample Modelcard for PMOS ********

** The BSIM-MG sample modelcard below was not extracted/obtained
** from/based on any real technologies. It should not be used for any
** other purposes except for benchmarking the implementation of BSIM-MG
** against BSIM Team's standard results

.model pmos1 PMOS level=17
+ AGIDL =3.000p
+ AGISL =3.000p
+ AIGBINV =11.10m
+ AIGC =13.60m
+ AT = 0.007
+ BG0SUB =1.120 
+ BGIDL =350.0E6
+ BGISL =350.0E6
+ BIGBINV =-1.000m
+ BIGC =1.710m
+ BULKMOD = 1
+ CDSC =13.00m
+ CDSCD =10.00m
+ CFS = 1.0e-10
+ CFD = 1.0e-10
+ CGEOMOD = 0
+ CGSL = 1.0e-10
+ CGDL = 1.0e-10
+ CIGBINV =6.000m
+ CIGC =75.00m
+ CIT =0.000  
+ CTH0 = 2.0e-5
+ DELTAW =0.000 
+ DELTAWCV =0.000 
+ TYPE = 0.000
+ DLC =0.000 
+ DROUT =0.530
+ DSUB =0.530
+ DVT0 =0.000
+ DVT1 =600.0m
+ EASUB =4.050 
+ EGIDL =0.000
+ EGISL =0.000
+ EIGBINV =1.100 
+ EOT = 1.0n
+ EPSROX =3.900 
+ EPSRSUB =11.90 
+ ETA0 =50.0m
+ ETAMOB =2.000
+ EU = 0.5
+ FECH =0.500 
+ FECHCV =1.000 
+ GEOMOD =1.000 
+ GIDLMOD =1.000 
+ HFIN = 30n
+ IGBMOD =1.000
+ IGCMOD =1.000
+ K1RSCE =0.000 
+ KSATIV =1.000
+ KT1 = 0.0
+ LINT =0.000 
+ LL =0.000
+ LLC =0.000 
+ LLN =1.000 
+ LPA =0.000
+ LPE0 =5.000n
+ MEXP = 3
+ NBODY = 1E+24
+ NC0SUB =2.86000E+25
+ NGATE = 0.0
+ NI0SUB =1.10000E+16
+ NIGBINV =3.000 
+ NSD =2.00000E+26
+ PCLM =5.000m
+ PDIBL1 = 0.300
+ PDIBL2 = 0.000
+ PHIN =50.00m
+ PHIG = 4.610
+ PRWGS = 0.000
+ PVAG = 0.000
+ QMFACTOR = 0.000 
+ RDSW = 100.0
+ RDSWMIN = 0.0
+ RSHS = 2.0
+ RTH0 = 0.05
+ U0 =20.00m
+ UA = 1.000
+ UA1 = 1.032m
+ UCS = 1.0
+ UD = 1.0
+ UP =0.000 
+ UTE = 0.000 
+ UTL =-1.497m
+ VSAT =150.0K
+ WR =1.000 
+ XL =-5n
+ IIMOD =0.0 
+ BETAII0 = 0
+ BETAII1 = .028   
+ BETAII2 = .067
+ TII = -0.7         
+ SII0 = 3.4  
+ SII1 = .8
+ SII2 = .08 
+ SIID = 0.08
+ ESATII = 1.7e6  
+ LII = 3e-9
+ RGATEMOD = 0
+ RGFIN = 100
+ NQSMOD = 0
+ RDSMOD = 0
+ SHMOD = 0
